**Highlights**

1. NO removal using active coke particles was investigated via numerical simulations.

2. A neural network model was developed to predict denitrification efficiency.

3. Key operating parameters were optimized to enhance denitrification performance.

4. The optimization significantly reduced costs and maintained effective denitrification.