

**Fig. 10****.** Effect of temperature on the outlet NO concentration.