

**Fig. 11****.** Effect of flow velocity on the outlet NO concentration.